(footprint "SPTA-1-4-3,5"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -6.35 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "d082e6ae-5280-4601-9456-f1329914c703")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SPTA-1-4-3,5"
		(at 0 6.35 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2599a274-5344-4f76-b5c4-92ca5a62656e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "SPTA-1-4-3,5"
		(at 0 -5.08 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b403e03d-8839-45fb-a9fd-0a849b82bf14")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5f66f5a4-a8fb-4363-b2e9-c47aabadaba6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e51cc530-eb80-48b6-be00-9365e988b0fd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -7.5 2.5)
		(end 7.5 2.5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0168388d-971d-4da2-9caa-cd1a1fa50e05")
	)
	(fp_line
		(start -7.5 3.5)
		(end 7.5 3.5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9211f3eb-94ed-411f-9a82-b6f6ace3accc")
	)
	(fp_rect
		(start -7.6 -4.3)
		(end 7.6 5.7)
		(stroke
			(width 0.15)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "63958327-5916-44be-852d-16b96e91faa2")
	)
	(pad "1" thru_hole oval
		(at -5.25 0)
		(size 2 3.5)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "aaacac04-f867-42d1-a67d-c331cdd0e1cf")
	)
	(pad "2" thru_hole oval
		(at -1.75 0)
		(size 2 3.5)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "aa484051-6948-4e2f-965c-48d448c37b40")
	)
	(pad "3" thru_hole oval
		(at 1.75 0)
		(size 2 3.5)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bdd4406b-59ac-43e7-8e76-921101e681fa")
	)
	(pad "4" thru_hole oval
		(at 5.25 0)
		(size 2 3.5)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "07fab500-f545-44c2-9562-6ae47e98e791")
	)
)
